Piper PA-28-181 Archer II_III — Roland_Bialy_PA28-181_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Before TAKE OFF" item count differs between passes (22 vs 23); verify nothing was dropped.
content_gap: Section "PRE - FLIGHT PA 28-181" item count differs between passes (12 vs 11); verify nothing was dropped.

PRE - FLIGHT PA 28-181
PREFLIGHT
[ ]  Seat Belts, Shoulder Harness .... ON
[ ]  Pax
[ ]  Radios / NAV / Avionics .... OFF
[ ]  Circuit Breakers .... IN
[ ]  Fuel selector .... FULLEST TANK
[ ]  Park Brake .... SET
[ ]  Flaps Full Range
[ ]  Trim
[ ]  Timer
[ ]  Freq XPDR ADF VOR BUGS .... SET
[ ]  Carb Heat .... OFF

Engine Start
[ ]  Primer
[ ]  Rotating Beacon .... ON
[ ]  Master Switch .... ON
[ ]  Prop Area .... CLEAR
[ ]  Electrical Fuel Pump .... ON
[ ]  Throttle .... 1/4 INCH OPEN
[ ]  Mixture .... RICH
[ ]  Starter .... ENGAGE
[ ]  Throttle .... ADJUST 800-1000 RPM
[ ]  Oil Press .... GREEN
[ ]  Mixture .... LEAN FOR TAXI
[ ]  Electrical Fuel Pump .... OFF
[ ]  Alternator
[ ]  Radio / Avionics .... ON
[ ]  Suction
[ ]  Annunciator Warn .... OFF
[ ]  A / P .... TEST
[ ]  Elec Trim .... TEST
[ ]  Gyro .... SET TO COMP
[ ]  Altimeter .... QNH
[ ]  XPDR .... STDBY
[ ]  Circuit Breakers .... ALL IN
[ ]  RPM
[ ]  Oil Press .... GREEN
[ ]  Fuel Qty / Selector .... AS CALC / FULLEST TANK
[ ]  Start UP / T H P .... CONFIRMED

TAXI
[ ]  Toe Brakes
[ ]  Bank Indicator / Gyro / Comp

RUN UP
[ ]  Park Brake .... SET
[ ]  Mixture .... FULL RICH
[ ]  Throttle .... 2000 RPM
[ ]  Oil Press .... GREEN
[ ]  Oil Temp .... GREEN
[ ]  MAGNETOS L / R max .... DELTA 50 DROP 175 RPM CHECKED
[ ]  Carb. Heat .... MAX DROP 100 RPM CHECKED
[ ]  Gyro Suction .... DROP IN LIMITS
[ ]  Alternator
[ ]  Throttle .... BACK TO IDLE - 1000 RPM
[ ]  Oil Press .... GREEN
[ ]  Oil Temp .... GREEN
[ ]  Annunciators .... TEST
[ ]  XPDR .... ON

Before TAKE OFF
[ ]  Flight Controls .... FREE AND CORRECT
[ ]  Altimeter .... SET
[ ]  GYRO .... SET
[ ]  Radios .... SET
[ ]  AVIONICS .... SET
[ ]  NAV BUGS .... SET
[ ]  Flaps .... AS REQRD
[ ]  Trim .... SET
[ ]  A / P .... OFF
[ ]  TAKE OFF BRIEFING
[ ]  EMERGENCY BRIEFING
[ ]  Window & Door .... SECURED
[ ]  PARK BRAKE .... OFF
[ ]  LINE UP .... READ BACK
[ ]  Fuel Pump .... ON
[ ]  RUNWAY .... LINE UP CENTER
[ ]  GYRO .... COMPASS IDENTICAL
[ ]  RUNWAY DESIGNATOR .... GYRO IDENTICAL
[ ]  XPDR .... ALTITUDE
[ ]  Landing Light .... ON
[ ]  Anti-Coll.-, NAV-Light / Pitot Heat .... AS REQRD
[ ]  TIME OFF
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