Piper PA-28-200R Arrow II — Steve_Koontz_1975_PA-28-200R_Arrow_WB
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Arrival Calculations" item count differs between passes (16 vs 15); verify nothing was dropped.
content_gap: Section "Departure Calculations" item count differs between passes (16 vs 15); verify nothing was dropped.

Departure Calculations
1975 PA-28-200R ARROW
WEIGHT / ARM / MOMENT
[ ]  Empty Weight .... 1640 / 84.7 / 138908
[ ]  Pilot & Front Pass .... 0 / 80.5 / 0
[ ]  Rear Seat Pass .... 0 / 118.1 / 0
[ ]  Usable Fuel (gal) - Tabs = 17 gal/tank .... 48 / 95 / 27360
[ ]  Baggage (200 lbs Max) .... 0 / 142.8 / 0
[ ]  Moment due to gear retraction .... 819
[ ]  Total (2750 lbs MAX) .... 1928 / 167087
[ ]  GROSS WEIGHT .... 1928
[ ]  CG .... 86.6633817427386
[ ]  Over/Under weight (lbs) .... 822 under gross
[ ]  Gallons/hour .... 11.5
[ ]  Time Aloft (hr) .... 4
[ ]  CG MIN .... 80.45607999999999
[ ]  CG MAX .... 93

Arrival Calculations
1975 PA-28-200R ARROW
WEIGHT / ARM / MOMENT
[ ]  Empty Weight .... 1640 / 84.7 / 138908
[ ]  Pilot & Front Pass .... 0 / 80.5 / 0
[ ]  Rear Seat Pass .... 0 / 118.1 / 0
[ ]  Usable Fuel Remaining (gal) .... 36 / 95 / 3420
[ ]  Baggage (200 lbs Max) .... 0 / 142.8 / 0
[ ]  Moment due to gear extension .... -819
[ ]  Total (2750 lbs MAX) .... 1676 / 141509
[ ]  GROSS WEIGHT .... 1676
[ ]  CG .... 84.43257756563246
[ ]  Over/Under weight (lbs) .... 1074 under gross
[ ]  Gallons/hour .... 11.5
[ ]  Reserve Time (hr) .... 0.5217391304347826
[ ]  CG MIN .... 80
[ ]  CG MAX .... 93

Aircraft Weight / CG Envelope
AIRCRAFT WEIGHT / CG MIN / CG MAX
[ ]  1500 .... 80 / 93
[ ]  1600 .... 80 / 93
[ ]  1700 .... 80 / 93
[ ]  1800 .... 80 / 93
[ ]  1900 .... 80.375 / 93
[ ]  1910 .... 80.41554 / 93
[ ]  1920 .... 80.45607999999999 / 93
[ ]  1930 .... 80.49661999999998 / 93
[ ]  1940 .... 80.53715999999997 / 93
[ ]  1950 .... 80.57769999999996 / 93
[ ]  1960 .... 80.61823999999996 / 93
[ ]  1970 .... 80.65877999999995 / 93
[ ]  1980 .... 80.69931999999994 / 93
[ ]  1990 .... 80.73985999999994 / 93
[ ]  2000 .... 80.78039999999993 / 93
[ ]  2010 .... 80.82093999999992 / 93
[ ]  2020 .... 80.86147999999991 / 93
[ ]  2030 .... 80.90201999999991 / 93
[ ]  2040 .... 80.9425599999999 / 93
[ ]  2050 .... 80.9830999999999 / 93
[ ]  2060 .... 81.02363999999989 / 93
[ ]  2070 .... 81.06417999999988 / 93
[ ]  2080 .... 81.10471999999987 / 93
[ ]  2090 .... 81.14525999999987 / 93
[ ]  2100 .... 81.18579999999986 / 93
[ ]  2110 .... 81.22633999999985 / 93
[ ]  2120 .... 81.26687999999984 / 93
[ ]  2130 .... 81.30741999999984 / 93
[ ]  2140 .... 81.34795999999983 / 93
[ ]  2150 .... 81.38849999999982 / 93
[ ]  2160 .... 81.42903999999982 / 93
[ ]  2170 .... 81.46957999999981 / 93
[ ]  2180 .... 81.5101199999998 / 93
[ ]  2190 .... 81.5506599999998 / 93
[ ]  2200 .... 81.59119999999979 / 93
[ ]  2210 .... 81.63173999999978 / 93
[ ]  2220 .... 81.67227999999977 / 93
[ ]  2230 .... 81.71281999999977 / 93
[ ]  2240 .... 81.75335999999976 / 93
[ ]  2250 .... 81.79389999999975 / 93
[ ]  2260 .... 81.83443999999974 / 93
[ ]  2270 .... 81.87497999999974 / 93
[ ]  2280 .... 81.91551999999973 / 93
[ ]  2290 .... 81.95605999999972 / 93
[ ]  2300 .... 81.99659999999972 / 93
[ ]  2310 .... 82.14659999999972 / 93
[ ]  2320 .... 82.29659999999973 / 93
[ ]  2330 .... 82.44659999999973 / 93
[ ]  2340 .... 82.59659999999974 / 93
[ ]  2350 .... 82.74659999999975 / 93
[ ]  2360 .... 82.89659999999975 / 93
[ ]  2370 .... 83.04659999999976 / 93
[ ]  2380 .... 83.19659999999976 / 93
[ ]  2390 .... 83.34659999999977 / 93
[ ]  2400 .... 83.49659999999977 / 93
[ ]  2410 .... 83.64659999999978 / 93
[ ]  2420 .... 83.79659999999978 / 93
[ ]  2430 .... 83.94659999999979 / 93
[ ]  2440 .... 84.0965999999998 / 93
[ ]  2450 .... 84.2465999999998 / 93
[ ]  2460 .... 84.39659999999981 / 93
[ ]  2470 .... 84.54659999999981 / 93
[ ]  2480 .... 84.69659999999982 / 93
[ ]  2490 .... 84.84659999999982 / 93
[ ]  2500 .... 84.99659999999983 / 93
[ ]  2510 .... 85.14659999999984 / 93
[ ]  2520 .... 85.29659999999984 / 93
[ ]  2530 .... 85.44659999999985 / 93
[ ]  2540 .... 85.59659999999985 / 93
[ ]  2550 .... 85.74659999999986 / 93
[ ]  2560 .... 85.89659999999986 / 93
[ ]  2570 .... 86.04659999999987 / 93
[ ]  2580 .... 86.19659999999988 / 93
[ ]  2590 .... 86.34659999999988 / 93
[ ]  2600 .... 86.49659999999989 / 93
[ ]  2610 .... 86.64659999999989 / 93
[ ]  2620 .... 86.7965999999999 / 93
[ ]  2630 .... 86.9465999999999 / 93
[ ]  2640 .... 87.09659999999991 / 93
[ ]  2650 .... 87.24659999999992 / 93
[ ]  2660 .... 87.39659999999992 / 93
[ ]  2670 .... 87.54659999999993 / 93
[ ]  2680 .... 87.69659999999993 / 93
[ ]  2690 .... 87.84659999999994 / 93
[ ]  2700 .... 87.99659999999994 / 93
[ ]  2710 .... 88.14659999999995 / 93
[ ]  2720 .... 88.29659999999996 / 93
[ ]  2730 .... 88.44659999999996 / 93
[ ]  2740 .... 88.59659999999997 / 93
[ ]  2750 .... 88.74659999999997 / 93
[ ]  2750 .... 93
[ ]  1500 .... 93

Weight and Balance Reference
[ ]  Envelope point 1500 .... 80 / 93
[ ]  TO location .... 1928
[ ]  Landing Loc .... 1676
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