Socata TB10 Tobago — Richard_Haines_Socata_tb10_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "11. Top of Descent Checks" item count differs between passes (8 vs 9); verify nothing was dropped.
content_gap: Section "12. D/wind Chk (BUMFFICHIW)" item count differs between passes (11 vs 12); verify nothing was dropped.
content_gap: Section "2. Before Start Checklist" item count differs between passes (3 vs 8); verify nothing was dropped.
content_gap: Section "6. Power/Run up Checklist" item count differs between passes (13 vs 14); verify nothing was dropped.
content_gap: Section "8. Take Off Checks" item count differs between passes (9 vs 10); verify nothing was dropped.

1. Cockpit checklist
[ ]  A/C documents .... ON-BOARD/CHKD
[ ]  Preflight /Logbook .... COMPLETED
[ ]  Ice/Weather .... REMOVED/CHECKED
[ ]  Control Lock/Tie dwn .... REMOVED
[ ]  Passenger Breifing .... GIVEN
[ ]  Doors/Seats/Belts .... LOCKED/CHKD
[ ]  All Switches/Radio .... OFF
[ ]  Brakes(park/foot) .... SET/ON
[ ]  Cockpit Checks Completed

2. Before Start Checklist
[ ]  Controls .... CHKD FULL & FREE
[ ]  Master Switch .... ON/CHECK HOBS
[ ]  Fuses .... CHKD IN

2a. Start up Clearance only
[ ]  Radio/Tower Freq .... ON/SET/CONTACT
[ ]  Start up Clearance .... RECEIVED
[ ]  Radio Master .... OFF
[ ]  Before Start Checks Complete

3. Starting Engine(master on)(COLD)
[ ]  Carb Heat .... COLD
[ ]  Propeller(blue) .... FWD
[ ]  Mixture .... RICH
[ ]  Fuel Tank(front panel) .... LOWEST TANK
[ ]  Fuel Pump(butt 1) .... ON/CHK PRESS
[ ]  Throttle Friction .... SET
[ ]  Throttle .... 2 PUMPS 1/4 OPEN
[ ]  Before Start .... CLEAR ALL ROUND
[ ]  Magnetos/Starter .... BOTH/ENGAGE
[ ]  Throttle .... 1000RPM(warm)
[ ]  Oil Pressure .... CHKD
[ ]  Engine Temp .... RISING
[ ]  Fuel Pump(butt 1) .... OFF
[ ]  Flaps .... UP

3a. Starting Engine (HOT)
[ ]  As above but .... NO Throttle pump
[ ]  Starting Engine Complete

4. After Start Checklist
[ ]  Generator(G) .... ON/CHKD
[ ]  Turn coordin(butt 3) .... ON
[ ]  Beacon/Nav lights .... ON
[ ]  Magnetos .... CHECK QUICKLY
[ ]  Ammeter/Suction .... CHGING/REGIST
[ ]  Compass/DI .... SET X-CHKD
[ ]  Radio nav/Autopilot .... SET/TEST/CHKD
[ ]  Radios/Tower .... ON/SET/CONTACT
[ ]  Altimeters .... SET QFE/QNH
[ ]  Transponder .... 7000 ON SBY
[ ]  CHECK TIME BRAKES OFF & NOTE
[ ]  FLIGHT PLAN OPENED ????
[ ]  After Start Checks complete

5. Taxi Checklist
[ ]  Control Column .... FULL BACK
[ ]  Brakes/rudder .... CHKD
[ ]  Turn indic/bal ball .... CHKD
[ ]  DI/Compass/AI .... CHKD
[ ]  Taxi check complete

6. Power/Run up Checklist
[ ]  Wheels/Action .... STRAIGHT/ LOOKOUT
[ ]  Brakes(foot/pking) .... FULL/HOLDING
[ ]  Engine Temp/Press .... GREEN ARC
[ ]  Fuel .... PUMP ON / FULLEST TANK
[ ]  Throttle .... 2000RPM
[ ]  Carb Heat .... CHECK
[ ]  Magnetos .... CHECK(175/50)
[ ]  Prop(Blue) .... BACK ONCE OIL
[ ]  Prop recycle .... BACK AGAIN CHECK
[ ]  Prop(controlling) .... CHECK WITH THROTTLE
[ ]  Suction/Ammeter .... CHECK
[ ]  Throttle .... IDLE CUT OUT CHECK THEN 1000RPM
[ ]  Power/Run up Check Completed

7. Before T/Off Checklist Vital Actions
[ ]  Trimmers .... SET FOR TAKE OFF
[ ]  Throttle Friction .... SET
[ ]  Mixture/Engine T&Ps .... RICH / WITHIN LIMITS
[ ]  Master/Magnetos .... MASTER ON/MAGS ON BOTH
[ ]  Pitot Heater .... AS REQUIRED
[ ]  Propeller .... FWD/FINE
[ ]  Fuel Pump .... ON
[ ]  Fuel .... FULLEST TANK
[ ]  Flaps .... T/O 10DEGS
[ ]  Instruments .... CHKD SET INC GPS
[ ]  Hatches/Harnesses .... CHKD SECURE
[ ]  Carb Heat .... RECHECK / COLD
[ ]  Controls .... FULL & FREE MOVEMENT
[ ]  Lights .... ALL ON
[ ]  Transponder .... 7000 ON ACS
[ ]  Radio Nav .... CHKD
[ ]  ATC Clearance .... RECEIVED
[ ]  Before T/Off Checks Complete

8. Take Off Checks
[ ]  Line up .... RWAY CLEAR / LOOKOUT
[ ]  Compass/DI .... X-CHKD RWAY HDING
[ ]  Brakes .... OFF
[ ]  Throttle .... HALF POWER
[ ]  Engine Temp/Press .... STEADY WITHIN LIMITS
[ ]  Throttle .... FULL POWER IF ABOVE OK
[ ]  Airspeed .... INCREASING
[ ]  Rotate .... FRONT WHEEL LIFT 50KNTS THEN MIN 65KNTS ROTATE
[ ]  Take Off Checks Complete

9. After T/Off Checklist(FLEETPI)>300'
[ ]  Flaps/Landing light .... UP / LANDING LIGHT OFF
[ ]  Engine Temp/Press .... STEADY WITHIN LIMITS
[ ]  Throttle/Prop .... 25"/2500RPM THROTTLE 1ST
[ ]  Attitude .... FOR BEST CLIMB 78KNTS
[ ]  Trimmer .... AS REQUIRED
[ ]  Altimeters .... CHKD SET QNH/QFE
[ ]  Fuel Pump .... OFF AT 1000' MIN CHK PRESS
[ ]  Icing .... CHECK SURFACES
[ ]  After T/Off Checks Complete

10. Top of Climb /Cruise Check
[ ]  Altitude .... SET / MAINTAIN
[ ]  Power/Prop .... ADJUST AS BELOW
[ ]  Trimmer .... AS REQUIRED
[ ]  Fuel .... CHANGE 15MINS
[ ]  Fuel Pump .... ON AS CHANGING
[ ]  Mixture .... ADJUST (EGTT)
NOTE: MAX 75% >1000'
[ ]  Engine .... T&Ps WITHIN LIMITS
[ ]  Instruments .... SET AS REQUIRED
[ ]  Compass/DI .... CHECK REGULARLY
[ ]  Icing .... CHECK SURFACES
[ ]  Weather .... CHECK WITH ATC
[ ]  Top of climb checks complete

11. Top of Descent Checks
[ ]  Radio / ATC .... FREQS / CONTACT
[ ]  Engine .... T&Ps WITHIN LIMITS
[ ]  Altimeter .... SET
[ ]  Radionav .... CHKD / CONFIRM
[ ]  Instrument Plates .... CHKD / CONFIRM
[ ]  Carb Heat .... HOT IF DESCENDG
[ ]  Power .... REDUCE THROTTLE TO APPROX 20"
[ ]  Top of Descent checks complete

12. D/wind Chk (BUMFFICHIW)
[ ]  ATC / Brakes .... CONTACT / OFF
[ ]  U/carriage / Speed .... FIXED / 100knots
[ ]  Master / Mags .... ON / BOTH
[ ]  Fuel pump .... ON/CHK PRESS
[ ]  Fuel Tanks .... FULLEST TANK
[ ]  Instruments .... QFE/NAV/T&Ps
[ ]  Carb heat .... CHKD
[ ]  Harnesses/Hatches .... SECURE/CLOSED
[ ]  Icing .... CHECK SURFACES
[ ]  Weather .... CHKD DIVERT IF REQUIRED
[ ]  Downwind Chk complete

13. Baseleg Checklist
[ ]  Throttle .... APPROX 15" MP
[ ]  Carb Heat .... HOT
[ ]  Flaps .... 10DEGS ONCE VFE(<95KNTS)
[ ]  Altitude .... IMC MINIMA
[ ]  Approach speed .... MIN 70 KNOTS
[ ]  Baseleg check complete

14. Finals Checks
[ ]  Landing Clearance .... RECEIVED
[ ]  Ldg Lights(whites) .... ON
[ ]  Mixture(red) .... RICH
[ ]  Propeller(Blues) .... FULLY FWD / FINE
[ ]  Throttle (black) .... SET FOR APPROACH SPEED
[ ]  Undercarriage(green) .... FIXED
[ ]  Fuel .... PUMP ON FULLEST TANK
[ ]  Carb Heat .... COLD @ 300FT
[ ]  Flaps .... FULL OVER THRESHOLD
[ ]  Finals Check Complete

15. After Landing Chks(once clear r/way)
[ ]  Carb Heat .... COLD
[ ]  Transponder .... OFF
[ ]  Fuel Pump/Pitot Ht .... OFF
[ ]  Landing Light .... OFF
[ ]  Flaps/Fuel Tanks .... UP/REFILL TO TABS
[ ]  After landing checks complete

16. Parking Checklist
[ ]  Brakes .... SET/Parking Brake ON
[ ]  CHECK TIME BRAKES ON & NOTE
[ ]  Radio Master .... OFF
[ ]  Throttle .... SET 1000 FOR 30 SECS
[ ]  Magnetos .... CHECK QUICKLY
[ ]  Throttle .... CLOSED
[ ]  Mixture .... CUT OFF
[ ]  All Switches/Fuel .... OFF / FUEL OFF SET CENTRE
[ ]  Master Switch .... OFF / CHECK HOBS
[ ]  Magnetos/Logbook .... OFF KEY OUT / COMPLETED
[ ]  Control Lock/Covers .... APPLIED / FIXED & SECURED
[ ]  Parking Checks completed

Notes and Performance Data
NOTE: NOTE:- CHECK TIME BRAKES OFF & ON & NOTE ON LOGSHEETS NOT HOBBS
NOTE: FLIGHT PLAN CLOSED ???
NOTE: FUEL (approx. 53US gallons usble. OIL-QTY-6-8Litres)
NOTE: CRUISE POWER SETTINGS — 2000ft 11oC MP IN 25/ 11.1 25/ 11.5 23.6/ 11 23.6/ 11.7 22.1/ 11.4; in.Hg/ 23.6/ 10.1 23.6/ 10.5 22.1/ 10 22.1/ 10.6 20.7/ 10.4; FUEL/HR 22.1/ 9.2 22.1/ 9.6 20.7/ 9.1 20.7/ 9.6 19.2/ 9.4; 20.7/ 8.4 20.7/ 8.7 19.2/ 8.4 19.2/ 8.8
NOTE: CRUISE POWER SETTINGS — 4000ft 7oC MP IN 23.6/ 10.4 23.6/ 10.9 23.6/ 11.4 23.6/ 12.1 22.1/ 11.8; in.Hg/ 22.1/ 9.6 22.1/ 9.9 22.1/ 10.3 22.1/ 11 20.7/ 10.7; FUEL/HR 20.7/ 8.7 20.7/ 9 20.7/ 9.7 20.7/ 9.9 19.2/ 9.7; 19.2/ 8.3 19.2/ 8.5 19.2/ 9.1
NOTE: CRUISE POWER SETTINGS — 6000ft 3oC MP IN 22.1/ 9.9 22.1/ 10.7 22.1/ 10.7 22.1/ 11.3 22.1/ 12.2; in.Hg/ 20.7/ 8.9 20.7/ 9.3 20.7/ 9.7 20.7/ 10.3 20.7/ 11.1; FUEL/HR 19.2/ 8.2 19.2/ 8.5 19.2/ 8.9 19.2/ 9.3 19.2/ 9.9
NOTE: CRUISE POWER SETTINGS — 8000ft -1oC MP IN 20.7/ 9.2 20.7/ 9.6 20.7/ 10 20.7/ 10.6 20.7/ 11.4; in.Hg/ 19.2/ 8.5 19.2/ 8.7 19.2/ 9.1 19.2/ 9.6 19.2/ 10.2; FUEL/HR 17.7/ 8.7 17.7/ 9.3
NOTE: CRUISE POWER SETTINGS — 10000ft -5oC MP IN 19.2/ 8.7 19.2/ 9 19.2/ 9.4 19.2/ 9.9 19.2/ 10.6; in.Hg/FB 17.7/ 9.5
NOTE: BOLD recommend figures head wind; BOLD recommend figures tail wind
NOTE: WEIGHTS — GROSS 2535Lbs, EMPTY 1500Lbs
NOTE: SPEEDS — KIAS / MPH: Vr rotation 65-75 / 75-90; Vy Best ROC 73 / 84; Vy 4up Best ROC 80 / 92; Vx Best AOC 67 / 78; Vfe Max Flaps 95 / 109; Va Cruise 115-122 / 140; Vno Struc CR 128 / 147; Vne Never exc 165 / 190; Ldng Normal 72-81 / 83-93; Ldng Soft/short 70 / 80; Glide BEST 86 / 99
NOTE: Add/decrease MP by 0.5 as temp varies 10°C above/below standard temp in table above
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